@page architecture  Architecture Overview


Modules
=======

The original architectural design of POV-Ray 3.7.0 identified POV-Ray as being comprised of two main entities, called
the _back-end_ and _front-end_. In a nutshell, the front-end would identify what scene file to render, start up one or
more back-end instances, make sure those have access to the input files, and let them parse the scene and subsequently
compute raw output image data from it. The front-end would then wait for the image data to trickle in, and ultimately
write the collected data to an actual image file. The communication between the front- and back-end would use a
proprietary asynchronous message-passing protocol called _POVMS_.

Each of these two entities resided in a separate sub-tree within the source tree, named `source/backend` and
`source/frontend`. A third sub-tree, `source/base`, contained code shared between back- and front-end.

@remark
    The ability to run and manage multiple back-end instances is a prerequisite for distributed rendering in a networked
    environment; however, to this date (2015-09-07), no official version of POV-Ray exists that implements this ability.
    As far as multi-core rendering is concerned, current implementations exclusively rely on multithreading support
    built into the back-end itself.

Current platform-specific implementations of POV-Ray also make use of another entity called the _virtual front-end_, or
_VFE_, the code of which resides outside the main source tree despite being shared across platforms. The purpose of this
entity is to abstract away various details of the _POVMS_ interface exposed by the official _front-end_.

Since the official release of POV-Ray 3.7.0, ongoing work has been put into further refining the architectural design,
currently distinguishing the following _modules_, each of which again resides in its own separate source sub-tree:


Back-End Module
---------------

The responsibility of the _back-end_ module, residing in the @ref source/backend source sub-tree, is being trimmed down
to coordinating multi-threaded execution of the _core_ and _parser_ modules, as well as interfacing them to a --
possibly remote -- _front-end_ instance via the _POVMS_ protocol.

@todo
    The exact line between the back-end module and the _core_ module has not been finalized yet.

The back-end module depends on the _base_, _core_, _parser_, _povms_ and _vm_ modules.


Base Module
-----------

The _base_ module, still residing in the @ref source/base source sub-tree, continues to be a loose collection of
miscellaneous utility code that happens to be shared across modules that should not interface directly, such as the
_core_ and _front-end_.

The base module is intended to be mostly unaware of multithreading, except that it makes provisions for sharing a few of
its data structures -- mostly related to performance optimizations -- among multiple threads.


Core Module
-----------

The _core_ module, residing in the @ref source/core source sub-tree, is designated to contain the actual render engine
code, the job of which is to take an internal representation of the scene and camera, and trace individual rays for
given pixel coordinates.

@todo
    The exact line between the core module and the _back-end_ module has not been finalized yet.

The core module is intended to be mostly unaware of multithreading, except that it makes provisions for sharing a few of
its data structures -- mostly related to performance optimizations -- among multiple core threads.

The core module depends on the _base_ module.

@note
    Although the core module makes use of the _vm_ module at run-time, the interface is entirely abstract, and
    therefore does not constitute a formal dependency. From the perspective of the core module, the vm module could be
    replaced any time with an entirely different implementation.


Front-End Module
----------------

The _front-end_ module, residing in the @ref source/frontend source sub-tree, currently retains its dual role of
providing high-level control of the rendering process as well as assembling the computed image data into an actual
result image file.

The front-end module depends on the _base_ and _povms_ modules.


Parser Module
-------------

The _parser_, residing in the @ref source/parser source sub-tree, is responsible for parsing a scene file, reading in
any auxiliary files such as include files and input images, and generating an internal representation of the scene and
camera in the format required by the _core_ module.

The parser module is entirely unaware of multithreading: It does not seem to make sense to run multiple parser instances
to process the same file, nor to share data between multiple parser instances processing different files.

The parser module depends on the _base_, _core_, and _vm_ modules.

@todo
    At present, the parser module also depends on the _back-end_ module.


POVMS Module
------------

The _POVMS_ module, residing in the @ref source/povms source sub-tree, implements the message-passing interface used
between the _front-end_ and _back-end_ modules.

The povms module depends on the _base_ module.


Virtual Machine Module {#module_vm}
----------------------

The _virtual machine_ module, or _VM_, residing in the @ref source/vm source sub-tree, implements a virtual machine to
execute user-defined functions, both during parsing and at render time.

The vm module depends on the _base_ and _core_ modules.


Platform-Specific Code {#module_sys}
----------------------

While the above modules are all designed to be portable, they rely on certain functionality that cannot be provided in a
portable manner, and consequently require platform-specific adapter code; in addition, for some functionality optimized
non-portable alternative implementations are provided. Such code resides in the separate @ref platform directory
sub-tree, even when conceptually considered part of one of the above modules.

@note
    Platform-specific code should not be confused with _user interface_-specific code.

@todo
    At present, some platform-specific code also resides in the @ref vfe directory sub-tree.


User Interface {#module_ui}
--------------

The above modules are started and controlled by the _user interface_.

@note
    POV-Ray does not provide any portable user interface; instead, each family of platforms has its own user interface,
    and potentially even multiple entirely different user interfaces (such as the GUI and command-line versions of
    POV-Ray for Windows).


Virtual Front-End Module
------------------------

The _virtual front-end_ module, or _VFE_, residing in the @ref vfe directory, contains code shared between several
user interfaces for POV-Ray, designed to abstract away various details of the _POVMS_ interface exposed by the
_front-end module_.


Units
=====

The POV-Ray code is comprised of hundreds of code _units_ -- that is, individual `.cpp` files and their respective
associated header files. Frequently, one unit corresponds to one C++ class, but this is not always the case. See the
file list for details on each individual file.
